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Prepared By (Carpenter Contractor)
Kansai Precision Carpentry Co., Ltd.
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Phone: +81-6-6211-4830
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Prepared For (Client)
Mr. Takashi Yamamoto
Address: 5-3-1 Namba, Chuo-ku, Osaka 556-0011, Japan
Phone: +81-90-5521-7743
Email: t.yamamoto@example.jp
Project Site: 12-7 Tennoji, Sumiyoshi-ku, Osaka 554-0031, Japan
1. Project Overview
This Quotation Estimate is issued by Kansai Precision Carpentry Co., Ltd. in response to the client's request for comprehensive Carpenter services to be performed at the residential property located in the Sumiyoshi-ku district of Japan Osaka. The scope of work encompasses structural woodwork, interior finishing, custom cabinetry, and exterior timber restoration. All materials and labor are sourced locally within the Japan Osaka metropolitan area to ensure quality control, timely delivery, and compliance with local building codes and regulations enforced by the Osaka City Construction Standards Office.
2. Scope of Work & Itemized Costs
	No.
	Description of Carpenter Work
	Unit
	Quantity
	Unit Price (JPY)
	Total (JPY)

	1
	Structural timber framing for second-floor extension (Hinoki cypress beams, 120mm x 200mm)
	Per m²
	45 m²
	18,500
	832,500

	2
	Custom built-in wardrobe and shelving unit (Kiri paulownia wood, 3.2m x 2.4m)
	Per set
	1 set
	485,000
	485,000

	3
	Interior wall paneling and wainscoting (Sugi cedar, tongue-and-groove)
	Per m²
	62 m²
	9,800
	607,600

	4
	Exterior veranda (engawa) restoration and re-laying of floor boards
	Per m²
	18 m²
	14,200
	255,600

	5
	Custom kitchen island with integrated sink cutout (Oak, 2.1m x 0.9m)
	Per unit
	1 unit
	320,000
	320,000

	6
	Staircase repair and handrail replacement (Hinoki, 12 risers)
	Per set
	1 set
	275,000
	275,000

	7
	Door frame and panel replacement (4 interior doors, Sugi cedar)
	Per door
	4 doors
	42,000
	168,000

	8
	Wooden flooring installation, living area (Sugi cedar, 15mm thick)
	Per m²
	38 m²
	11,500
	437,000

	9
	Site preparation, material handling, and debris removal
	Per day
	12 days
	28,000
	336,000

	10
	Final sanding, staining, and natural oil finish application
	Per m²
	120 m²
	3,200
	384,000

	Subtotal (Labor + Materials)
	4,100,700

	Consumable Materials (fasteners, adhesives, sandpaper, sealants)
	186,500

	Consumable Tax (10% JCT)
	428,720

	GRAND TOTAL
	4,715,920 JPY


3. Project Timeline
The Carpenter team assigned to this project in Japan Osaka consists of one master carpenter (Shokunin), two skilled journeymen, and one apprentice. The estimated duration of the project is 22 working days, commencing on 1 July 2025 and concluding by 28 July 2025, subject to weather conditions and material availability. A detailed weekly schedule will be provided upon acceptance of this Quotation Estimate.
4. Terms and Conditions
4.1 This Quotation Estimate is valid for thirty (30) calendar days from the date of issue. After the expiry date, all prices are subject to revision based on current lumber market rates in the Japan Osaka region.
4.2 Payment shall be made in three installments: 30% upon contract signing, 40% upon completion of structural framing, and 30% upon final inspection and handover. All payments are to be made in Japanese Yen (JPY) via bank transfer to the account specified in the contract.
4.3 The Carpenter contractor guarantees all workmanship for a period of two (2) years from the date of completion. This warranty covers structural integrity, joinery, and finish defects but does not cover damage caused by natural disasters, improper use, or third-party modifications.
4.4 All materials used shall comply with the Japanese Industrial Standards (JIS) for timber products. The Carpenter team will provide material certificates and FSC (Forest Stewardship Council) documentation upon request.
4.5 The client is responsible for obtaining all necessary permits from the Osaka City Building Standards Division prior to the commencement of structural work. The Carpenter contractor will assist in preparing technical drawings for permit submission at no additional cost.
4.6 Any changes to the scope of work requested by the client after this Quotation Estimate has been accepted will be subject to a written change order with revised pricing and timeline adjustments.
4.7 The Carpenter contractor maintains full liability insurance and workers' compensation coverage as required by Japanese law. Proof of insurance will be provided upon request.
4.8 Disputes arising from this agreement shall be resolved through mediation in accordance with the Osaka District Court jurisdiction.
5. Acceptance
By signing below, the client acknowledges receipt of this Quotation Estimate and agrees to the terms, conditions, and pricing outlined herein for the Carpenter services to be performed in Japan Osaka. This document, once countersigned by both parties, constitutes a binding agreement.
For Kansai Precision Carpentry Co., Ltd.
Master Carpenter / Project Lead
Name: Kenji Sato
Signature & Company Seal (Hanko)
Date: _______________
For the Client
Property Owner
Name: Takashi Yamamoto
Signature
Date: _______________
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