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	Quotation Estimate No.:
	QTE-MASON-CAS-2025-0347
	Date of Issue:
	15 June 2025

	Project Location:
	Quartier Gauthier, Morocco Casablanca
	Validity Period:
	30 days from issue date

	Project Type:
	Residential Masonry & Structural Work
	Estimated Duration:
	45 working days


1. Scope of Mason Work – Morocco Casablanca
This Quotation Estimate is issued by Atlas Mason & Construction Services SARL, a fully licensed and insured Mason operating in Morocco Casablanca, to provide a comprehensive breakdown of all masonry, structural, and finishing works required for the client's residential property. The Mason team will execute all tasks in strict compliance with Moroccan building regulations (Réglementation de Construction) and the specific urban planning codes applicable to the Casablanca metropolitan area.
· Foundation Masonry: Excavation, formwork, and concrete pouring for strip foundations (1.2m depth) using C25/30 concrete, reinforced with HA12 and HA16 steel bars, in accordance with Moroccan seismic zone requirements for Casablanca.
· Load-Bearing Wall Construction: Erection of 20cm thick load-bearing walls using standard Moroccan clay bricks (briques de terre cuite) with M10 cement mortar, including proper bonding patterns and reinforcement at corners and openings.
· Partition Walls: Construction of 10cm non-load-bearing partition walls using hollow concrete blocks (parpaings) for interior room divisions throughout the ground floor and first floor.
· Lintels & Structural Openings: Installation of precast concrete lintels (25cm x 15cm) above all door and window openings, with proper bearing of minimum 25cm on each side.
· Staircase Masonry: Construction of a straight-run concrete staircase (14 steps) with brickwork stringers, including handrail anchoring points and nosing finishing.
· Plastering & Rendering: Application of two-coat cement plaster (1.5cm + 1cm) on all interior and exterior masonry surfaces, followed by a smooth finishing coat on exterior walls.
· Chimney & Ventilation Shafts: Masonry construction of one kitchen chimney (20cm x 20cm) and two bathroom ventilation shafts using fire-rated bricks and refractory mortar.
· Site Cleanup & Debris Removal: Complete removal of all construction waste, broken bricks, and masonry debris from the site in Morocco Casablanca, in compliance with local waste disposal regulations.
2. Itemized Cost Breakdown
	Item No.
	Description of Mason Work
	Unit
	Quantity
	Unit Price (MAD)
	Total (MAD)

	01
	Foundation masonry & concrete works (C25/30, reinforced)
	m³
	18.5
	2,850
	52,725.00

	02
	Load-bearing brick walls (20cm, clay bricks, M10 mortar)
	m²
	142.0
	385
	54,670.00

	03
	Interior partition walls (10cm, hollow blocks)
	m²
	96.0
	245
	23,520.00

	04
	Precast concrete lintels (25cm x 15cm) – supply & install
	Unit
	14
	1,250
	17,500.00

	05
	Concrete staircase masonry (14 steps, brick stringers)
	Lot
	1
	48,500
	48,500.00

	06
	Interior & exterior plastering (two-coat cement render)
	m²
	420.0
	125
	52,500.00

	07
	Chimney & ventilation shaft masonry (fire-rated)
	Lot
	1
	12,800
	12,800.00

	08
	Scaffolding, formwork, and temporary works
	Lot
	1
	15,200
	15,200.00

	09
	Site cleanup, debris removal & waste disposal (Casablanca)
	Lot
	1
	8,500
	8,500.00

	10
	Mason supervision, project management & quality control
	Lot
	1
	18,000
	18,000.00

	Subtotal (MAD)
	303,915.00

	TVA 20% (Moroccan Value Added Tax)
	60,783.00

	GRAND TOTAL (MAD)
	364,698.00


* All prices are quoted in Moroccan Dirhams (MAD). The Mason contractor assumes responsibility for all labor, standard materials, and equipment. Special materials or design modifications requested by the client after this Quotation Estimate is accepted will be subject to a separate supplementary quotation.
3. Payment Schedule
This Quotation Estimate for Mason services in Morocco Casablanca shall be settled according to the following milestone-based payment plan:
· Advance Payment (30%): MAD 109,409.40 – Due upon signing of the contract and acceptance of this Quotation Estimate.
· Progress Payment 1 (30%): MAD 109,409.40 – Due upon completion of foundation and load-bearing wall masonry.
· Progress Payment 2 (25%): MAD 91,174.50 – Due upon completion of partition walls, staircase, and lintel installation.
· Final Payment (15%): MAD 54,704.70 – Due upon final handover, site cleanup, and client sign-off.
4. Terms & Conditions
4.1 This Quotation Estimate is valid for a period of thirty (30) calendar days from the date of issue. After this period, the Mason contractor reserves the right to revise pricing due to material cost fluctuations in the Morocco Casablanca market.
4.2 The estimated project duration of forty-five (45) working days assumes standard weather conditions and uninterrupted access to the site in Morocco Casablanca. Delays caused by force majeure, client-requested changes, or regulatory holds by the Casablanca urban planning authority (Direction de l'Urbanisme) shall extend the timeline accordingly.
4.3 The Mason contractor guarantees all masonry work for a period of two (2) years from the date of final acceptance, covering structural defects, improper bonding, and material failures attributable to workmanship.
4.4 The client is responsible for obtaining all necessary building permits (permis de construire) from the Mairie de Casablanca prior to the commencement of any Mason work. The Mason contractor shall provide all technical drawings and structural calculations required for the permit application at no additional cost.
4.5 All work shall comply with the Moroccan building code (Réglementation de Construction), seismic regulations applicable to Casablanca (Zone Seismique IIb), and local Casablanca urban planning directives.
4.6 Any dispute arising from this Quotation Estimate or the subsequent contract shall be resolved through amicable negotiation. Failing resolution within thirty (30) days, the matter shall be submitted to the competent courts of Casablanca, Morocco.
4.7 The Mason contractor maintains full civil liability insurance and workers' compensation coverage as required by Moroccan law. Certificates of insurance are available upon request.
5. Acceptance & Signatures
By signing below, both parties acknowledge and agree to the terms, scope, and pricing outlined in this Quotation Estimate for Mason services to be executed in Morocco Casablanca. This document, once signed, constitutes a binding agreement between the parties.
Client Signature
Mr. Youssef El Amrani
Date: _______________
Mason Contractor Signature
Atlas Mason & Construction Services SARL
Authorized Representative
Date: _______________
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