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Quotation Estimate
Quotation Details
Quotation No.: QTE-KPL-2025-0847
Date Issued: 14 June 2025
Valid Until: 14 July 2025 (30 days)
Project Location: Kampala, Uganda
Client Information
Client Name: Mr. David Okello
Address: Plot 14, Ntinda Road, Kampala, Uganda
Contact: +256 701 987 654
Email: d.okello@email.com
Dear Mr. Okello,
Thank you for your enquiry regarding masonry and structural construction services in Uganda Kampala. This Quotation Estimate has been prepared by our experienced Mason team to provide you with a comprehensive and transparent breakdown of all costs associated with the proposed masonry works at your residential property in Ntinda, Kampala. Our Mason crew has assessed the site on 10 June 2025 and this Quotation Estimate reflects the full scope of work required to complete the project to the highest standards of Ugandan building codes and regulations.
Scope of Mason Work
This Quotation Estimate covers the complete masonry construction of a two-storey residential building in Uganda Kampala, including foundation walls, ground floor and first floor blockwork, lintels, columns, and finishing. Our lead Mason, with over 18 years of experience in Kampala's construction industry, will supervise all works personally. The masonry works will be executed using standard 9-inch and 6-inch concrete blocks sourced from approved suppliers within Kampala district.
Itemized Cost Breakdown
	Item No.
	Description of Mason Work
	Unit
	Quantity
	Unit Rate (UGX)
	Amount (UGX)

	1
	Foundation wall masonry (9-inch blocks, cement mortar 1:4)
	m²
	185
	45,000
	8,325,000

	2
	Ground floor external wall masonry (9-inch blocks)
	m²
	320
	52,000
	16,640,000

	3
	Ground floor internal partition walls (6-inch blocks)
	m²
	210
	38,000
	7,980,000

	4
	First floor external wall masonry (9-inch blocks)
	m²
	295
	55,000
	16,225,000

	5
	First floor internal partition walls (6-inch blocks)
	m²
	195
	40,000
	7,800,000

	6
	Reinforced concrete lintels (door and window openings)
	nos
	28
	85,000
	2,380,000

	7
	Reinforced concrete columns (400mm x 400mm, C25 concrete)
	nos
	16
	450,000
	7,200,000

	8
	Ring beam and roof slab edge masonry
	m
	96
	65,000
	6,240,000

	9
	Internal plastering (both sides, 12mm thick, cement:sand 1:3)
	m²
	1,200
	28,000
	33,600,000

	10
	External plastering and rendering (weatherproof finish)
	m²
	615
	35,000
	21,525,000

	11
	Scaffolding, formwork, and temporary works
	lump sum
	1
	3,500,000
	3,500,000

	12
	Site supervision by senior Mason and project engineer
	months
	5
	1,200,000
	6,000,000

	TOTAL ESTIMATED COST (UGX)
	137,415,000


Grand Total in Ugandan Shillings: UGX 137,415,000 (One Hundred and Thirty-Seven Million, Four Hundred and Fifteen Thousand Ugandan Shillings Only)
Approximate USD Equivalent: USD 36,800 (at prevailing exchange rate)
Payment Schedule
This Quotation Estimate for masonry works in Uganda Kampala is structured with the following milestone-based payment plan to ensure transparency and mutual confidence between our Mason team and the client:
	Milestone
	Percentage
	Amount (UGX)
	Trigger

	Advance / Mobilization
	20%
	27,483,000
	Upon signing of contract

	Foundation & Ground Floor Walls Complete
	30%
	41,224,500
	Inspection sign-off

	First Floor Walls & Lintels Complete
	25%
	34,353,750
	Inspection sign-off

	Plastering & Finishing Complete
	20%
	27,483,000
	Final inspection

	Retention / Defects Liability
	5%
	6,870,750
	After 90-day defect period


Terms and Conditions
1. This Quotation Estimate is valid for thirty (30) calendar days from the date of issue. Prices are subject to revision after the expiry date due to fluctuations in material costs in the Kampala market.
1. All masonry works will be carried out in strict compliance with the Uganda National Building Regulations and the Kampala Capital City Authority (KCCA) building bylaws.
1. The Mason team shall provide all labour, tools, and small equipment. The client is responsible for the supply of major materials (cement, blocks, sand, aggregate, and reinforcement steel) unless otherwise agreed in writing.
1. The estimated project duration is five (5) months from the date of commencement, subject to weather conditions and timely availability of materials in Uganda Kampala.
1. Any variation or additional masonry work beyond the scope described in this Quotation Estimate shall be subject to a separate written variation order signed by both parties.
1. The Mason contractor shall maintain adequate insurance coverage for workmen's compensation and third-party liability throughout the duration of the project.
1. Disputes arising from this Quotation Estimate or the resulting contract shall be resolved through mediation in Kampala, Uganda, in accordance with the Arbitration Act of Uganda.
1. The client shall provide safe access to the site, adequate water supply, and temporary power connections to facilitate the masonry works.
1. A defects liability period of ninety (90) days shall apply from the date of practical completion, during which the Mason team shall rectify any defects in masonry workmanship at no additional cost.
Acceptance and Authorization
By signing below, the client acknowledges receipt of this Quotation Estimate for masonry services in Uganda Kampala and agrees to the terms, conditions, and pricing outlined herein. The Mason contractor commits to delivering all works to the specified standards and within the agreed timeline.
For: Kampala Mason & Construction Services Ltd.
Name: Eng. Samuel Mukasa (Lead Mason / Project Director)
Signature: _________________________
Date: _________________________
For: The Client
Name: Mr. David Okello
Signature: _________________________
Date: _________________________
Kampala Mason & Construction Services Ltd. | P.O. Box 4521, Kampala, Uganda
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